INSTALL README - ERAD TOUCH DATA LOGGER
Step 1:	Determine whether the computer is running the SQLite or SQL Server Express version of the Datalogger. This can be done by doing the following:
a.	Open up the currently installed ERAD Touch Datalogger.
b.	Click on the "Help" drop-down menu and select "About".
c.	In the window that pops up scroll down to the bottom in the whited out section.
d.	At the bottom of the whited out section there is a line called "Database: SQLxxxxxxx". Here it will tell you whether you have SQLite (fig 1) or SQL Server Express (fig2).

Figure 1: About window SQLite Version.

Figure 2: About window SQLite Server Express Version.

Step 2: Download the ERAD Touch Datalogger Version based on Step 1.

Step 3: Un-install the old version of the ERAD Touch Datalogger. The existing Database will not be removed and can be viewed once the new ERAD Touch Datalogger is installed.
Warning!! Failure to un-install the old version before installing the new version will result in a corrupt and un-viewable Database.

Step 4: Run the "setup.exe" found in the downloaded ZIP file to install the ERAD Touch Datalogger. 

Step 5: Download hardware drivers from the download section of: www.eradtorque.com. There is one for x64 Systems and one for x84 Systems. If unsure which system you have just download and try installing one, a message will pop up to let you know if it is incorrect in which case just download the other and install it.
Warning!! Failure to install the new drivers will result in wired communication issues.